**Personal Protective Equipment and Clothing.**

**DO NOT** use this machine unless you have been instructed in its safe use and

operation and have been given permission.

**This safe Operating Procedure does not necessarily cover all possible hazards associated with this equipment and should be used in conjunction with the manufacturer’s guidance. It is designed as a guide to be used to compliment training and as a reminder to users prior to equipment use. Users acknowledge that improper use of equipment increases their risk of harm and that this is a decision they make. Anyone found to be using equipment incorrectly will have their usage rights removed pending a re-training exercise on the safe use of the equipment.**

**Finishing Operations and Housekeeping.**

**🗸** Ensure sufficient time for materials to cool before handling.

**🗸** Ensure the welder is switched off (and fume extraction if used).

**🗸** Check for any damage to welder and cables at the end of job. Wind up cables.

**🗸** Hang up the welding handpiece and cables securely.

Check contact points for damage corrosion.

**🗸** Leave the machine in a safe, clean, and tidy state.

**Operational Safety Checks.**

**🗸** Ensure task in hand is clearly understood.

**🗸** Ensure the welder is correctly set up for current, voltage & good earth.

**🗸** Ensure that other workers in this locality are protected from any UV & IR radiation flash. Always close the UV curtain to the welding bay or erect a UV screen.

**🗸** Ensure appropriate ventilation is in place prior to use as welding aluminium, zinc etc will release harmful fumes.

**🗸** Ensure the welding return cable (earth) makes firm contact to provide a good electrical contact.

**🗸** Ensure your workpiece has been prepared to be free of any paint, oxides or other surface finishes ensuring a good electrical contact.

**🗸** Take particular care to avoid accidental UV welding flash to the skin or eyes.

**🗸** Never leave the welder running unattended.

Regularly inspect the welding tip and shield for damage.

**🗸** When welding is finished or interrupted, turn off the welder and secure the handpiece safely.

**🗸** Ensure the work area can isolate hot areas from workers to avoid hot surfaces until job is cool.

**Potential Hazards and Injuries.**

**¡** Electrocution.

**¡** Burns to eyes or body.

**¡** Inhalation of fumes.

**¡** Damage to eyes.

**¡** Flying sparks.

**¡** Fire.

**¡** Cuts & lacerations.

**¡** Slips, Trips and Falls.

**Pre-Operational Safety checks.**

**🗸** Ensure the welder is used in a suitable safe work area.

**🗸** Ensure all cables are correctly fastened, free of cracks and splits and unwound before work.

**🗸** Keep the area clean and free of grease, oils & flammable materials.

**🗸** Ensure other workers are protected from any UV flash.

**🗸** Ensure the area is well ventilated (with fume extraction as required).

**Don’t.**

X Do not use faulty equipment. Immediately report any suspect machinery.

X Never leave the machine running attended.

|  |  |  |  |
| --- | --- | --- | --- |
| A\* | *For use by trained staff only. Use by anyone else strictly prohibited.* | A | *For use by adult employees (18+) who have received and signed the safe use paperwork. No lone working.* |
| B | *For use by adult employees (16+) who have received and signed the safe use paperwork. Lone working Permitted.* | C | *For use by all employees under the supervision of adult employees who have received and signed the safe use paperwork. Adult lone working permitted.* |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Welding Mask Safety Signs - from Key Signs UK | Appropriate welding mask with correct grade lens to be worn. | WEAR DUST MASK PROTECTION SAFETY SYMBOL SELF ADHESIVE VINYL STICKERS SAFETY  | eBay | Dust mask or other RPE must be worn. |  | Jewellery & watches forbidden. |
| Wear Safety Boots Signs - from Key Signs UK | Safety footwear must be worn at all times in work areas. | ISO Safety Gloves Required Sign, SKU: IS-1008 | Safety gloves must be worn when using this equipment. |  | Fire resistant protective clothing to be worn. |
| Safety operating procedures | Long & loose hair must be contained. |  |